|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| **WARNING** | | | | | |
| **LASER CONTROLLED AREA** | | | | | |
|  | **LASER**  **Class 3B & 4** | |  | |  |
| *Invisible and Visible Laser Radiation* | | | Avoid eye or skin exposure to direct and/or scattered radiation | | |
| |  |  |  |  |  | | --- | --- | --- | --- | --- | | **Laser System**  **Designation** | **Emitted Wavelength (nm)** | **Max. Output Power (W)** | **Max Energy per Pulse (mJ)** | **Required Optical Density** | | Thorlabs L375P070MLD | 375 | 70 - 85 mW | - | OD 3 | | Nichia NDV 4622 | 405 | 100 - 250 W | - | OD 3 | |  |  |  |  |  | |  |  |  |  |  | | | | | | |
| **Laser Safety Contact** | | XXX | | 808 XXXX | 054 XXX XXXX |
| **Laser Safety Officer** | | Delphine Darios | | 808 2206 | 054 470 0564 |

**Edit Text in Red**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Laser System**  **Designation** | **Emitted Wavelength (nm)** | **Max. Output Power (W)** | **Max Energy per Pulse (mJ)** | **Required Optical Density** |
| Thorlabs L375P070MLD | 375 | 70 - 85 mW | - | OD 3 |
| Nichia NDV 4622 | 405 | 100 - 250 W | - | OD 3 |
|  |  |  |  |  |
|  |  |  |  |  |